SPLP has made revisions to the proposed workspaces in Perry County since submittal of the original application.  These revisions have been the result of landowner requests, agency requests, the avoidance of sensitive species or their habitats, and/or to further reduce impacts to aquatic resources.  The additions and subtractions to the workspaces are listed and quantified within Table 1.  In addition, this attachment highlights the location and extent of these additions and subtractions to the workspaces on a set of site plans.  Each addition/subtraction has been assigned an identification code and that code is reflected below and on the set of site plans.  The additions and subtractions are listed from west to east. A total of approximately 11.63 acres was added and 8.38 acres subtracted for a net increase of 3.25 acres of earth disturbance.

**Table 1.  Pennsylvania Pipeline Project LOD Additions and Subtractions.**

| **CHANGE ID** | **COUNTY** | **REASON FOR CHANGE** | **ACREAGE** | **LOD ADDITION OR SUBTRACTION** | **WETLAND DELINEATION1** | **PNDI EVALUATION2** | **SHEET NUMBER** | **E&S SHEET NUMBER** |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Doylesburg Station | PERRY | Station design | 1.68 | Addition | Yes | YesA | 6 | 3.09 |
| Sub-115 | PERRY | Minor LOD adjustment needed to facilitate safe installation | 0.21 | Subtraction | NA | NA | 2 | 3.03 |
| Add-92 | PERRY | Temporary Access Road reroute to facilitate installation. No additional aquatic resources impacted. | 0.39 | Addition | Yes | YesA | 2 | 3.03 |
| Sub-116 | PERRY | Minor LOD adjustment needed to facilitate safe installation | 0.01 | Subtraction | NA | NA | 6 | 3.09 |
| Sub-117 | PERRY | Minor LOD adjustment needed to facilitate safe installation | 0.01 | Subtraction | NA | NA | 6 | 3.09 |
| Add-93 | PERRY | Additional LOD added for Doylesburg Pump Station connection lines. | 0.51 | Addition | Yes | YesA | 6 | 3.10 |
| Sub-118 | PERRY | Minor LOD adjustment needed to facilitate safe installation | 0.01 | Subtraction | NA | NA | 6 | 3.10 |
| Add-94 | PERRY | Minor shift to accommodate avoidance of adjacent property line. Minor increase in wetland and stream impacts. | 0.23 | Addition | Yes | YesA | 6 | 3.10 |
| Sub-119 | PERRY | Minor LOD adjustment needed to facilitate safe installation | 0.02 | Subtraction | NA | NA | 6 | 3.10 |
| Add-95 | PERRY | PA DCNR Requested minor shift to avoid endangered plant area. | 0.43 | Addition | Yes | YesA | 9 | 3.14 |
| Sub-120 | PERRY | Minor LOD adjustment needed to facilitate avoidance of a sensitive plant population | 0.01 | Subtraction | NA | NA | 9 | 3.15 |
| Add-96 | PERRY | PA DCNR Requested minor shift to avoid endangered plant area. | 0.23 | Addition | Yes | YesA | 9 | 3.15 |
| Add-97 | PERRY | Minor LOD adjustment needed to facilitate safe installation | 0.04 | Addition | Yes | YesA | 10 | 3.15 |
| Add-98 | PERRY | PA DCNR Requested minor shift to avoid endangered plant area. | 0.37 | Addition | Yes | YesA | 10 | 3.14 |
| Add-99 | PERRY | PA DCNR Requested minor shift to avoid endangered plant area. | 0.19 | Addition | Yes | YesA | 10 | 3.16 |
| Sub-121 | PERRY | Minor LOD adjustment needed to facilitate safe installation | 0.09 | Subtraction | NA | NA | 10 | 3.16 |
| Sub-122 | PERRY | Reroute to avoid cultural resources. Also reduction in wetland impacts. | 1.11 | Subtraction | NA | NA | 14 | 3.22 |
| Add-100 | PERRY | Reroute to avoid a cultural area located to the south. Also resulted in a reduction of wetland impacts. | 1.26 | Addition | Yes | YesA | 14 | 3.22 |
| Sub-123 | PERRY | Minor LOD adjustment needed to facilitate safe installation | 0.05 | Subtraction | NA | NA | 16 | 3.26 |
| Sub-124 | PERRY | Minor LOD adjustment needed to facilitate safe installation | 0.30 | Subtraction | NA | NA | 16 | 3.26 |
| Add-101 | PERRY | PA DCNR requested alignment stay to south of existing 8-inch line in this area to protect woodrat and rattlesnake habitat | 0.16 | Addition | Yes | YesA | 16 | 3.26 |
| Add-102 | PERRY | PA DCNR requested alignment stay to south of existing 8-inch line in this area to protect woodrat and rattlesnake habitat | 4.01 | Addition | Yes | YesA | 17 | 3.27 |
| Sub-125 | PERRY | PA DCNR requested alignment stay to south of existing 8-inch line in this area to protect woodrat and rattlesnake habitat | 4.41 | Subtraction | NA | NA | 17 | 3.27 |
| Add-103 | PERRY | PA DCNR requested alignment stay to south of existing 8-inch line in this area to protect woodrat and rattlesnake habitat | 2.13 | Addition | Yes | YesA | 17 | 3.28 |
| Sub-126 | PERRY | PA DCNR requested alignment stay to south of existing 8-inch line in this area to protect woodrat and rattlesnake habitat | 2.15 | Subtraction | NA | NA | 18 | 3.28 |

1 – The added area was field investigated for aquatic resources. Not applicable is listed for LOD subtractions.

2 – The added area was originally evaluated for PNDIA or PNDI was revisited through interim correspondence and analysisB. Not applicable is listed for LOD subtractions.